


LAB-4


1. Configuring Default Route

Topology:











2.Configuring RIP protocol to a router


Topology:




For Router1



For Router2





For Router3




Output:

End Device with ip address 10.0.0.10







End Device with ip address 40.0.0.10

